
Loading device database for application reportgen from file
"simple1_clk_wrapper.ncd".
   "simple1_clk_wrapper" is an NCD, version 2.38, device xc2s50, package pq208,
speed -6
Loading device for application reportgen from file 'v50.nph' in environment
C:/xilinx_62i.
Device speed data version:  PRODUCTION 1.27 2003-12-13.

Generating Delay Report: simple1_clk_wrapper.dly


   The Delay Summary Report

   The SCORE FOR THIS DESIGN is: 183


The NUMBER OF SIGNALS NOT COMPLETELY ROUTED for this design is: 0

   The AVERAGE CONNECTION DELAY for this design is:        1.327
   The MAXIMUM PIN DELAY IS:                               3.000
   The AVERAGE CONNECTION DELAY on the 10 WORST NETS is:   2.515

   Listing Pin Delays by value: (nsec)

    d < 1.00   < d < 2.00  < d < 3.00  < d < 4.00  < d < 5.00  d >= 5.00
   ---------   ---------   ---------   ---------   ---------   ---------
         229         530         107           1           0           0


reportgen done!
