#PACE: Start of Constraints generated by PACE

#PACE: Start of PACE I/O Pin Assignments
NET "anode1"  LOC = "p69"  ;
NET "anode2"  LOC = "p71"  ;
NET "anode3"  LOC = "p75"  ;
NET "cathode<0>"  LOC = "p74"  ;
NET "cathode<1>"  LOC = "p70"  ;
NET "cathode<2>"  LOC = "p67"  ;
NET "cathode<3>"  LOC = "p62"  ;
NET "cathode<4>"  LOC = "p61"  ;
NET "cathode<5>"  LOC = "p73"  ;
NET "cathode<6>"  LOC = "p68"  ;
NET "cathode<7>"  LOC = "p63"  ;
NET "clock"  LOC = "p77"  ;
NET "in_x_0<10>"  LOC = "p82"  ;
NET "in_x_0<11>"  LOC = "p81"  ;
NET "in_x_0<12>"  LOC = "p168"  ;
NET "in_x_0<13>"  LOC = "p166"  ;
NET "in_x_0<14>"  LOC = "p164"  ;
NET "in_x_0<15>"  LOC = "p162"  ;
NET "in_x_0<1>"  LOC = "p180"  ;
NET "in_x_0<2>"  LOC = "p178"  ;
NET "in_x_0<3>"  LOC = "p175"  ;
NET "in_x_0<4>"  LOC = "p89"  ;
NET "in_x_0<5>"  LOC = "p88"  ;
NET "in_x_0<6>"  LOC = "p87"  ;
NET "in_x_0<7>"  LOC = "p86"  ;
NET "in_x_0<8>"  LOC = "p84"  ;
NET "in_x_0<9>"  LOC = "p83"  ;
NET "reset"  LOC = "p59"  ;

#PACE: Start of PACE Area Constraints

#PACE: Start of PACE Prohibit Constraints

#PACE: End of Constraints generated by PACE
