Release 6.2i Par G.28
Copyright (c) 1995-2004 Xilinx, Inc.  All rights reserved.

TPSDP::  Sun Aug 21 16:15:32 2005


C:/xilinx_62i/bin/nt/par.exe -w -intstyle ise -ol std -t 1 counter_map.ncd
counter.ncd counter.pcf 


Constraints file: counter.pcf

Loading device database for application Par from file "counter_map.ncd".
   "counter" is an NCD, version 2.38, device xc2s50, package pq208, speed -6
Loading device for application Par from file 'v50.nph' in environment
C:/xilinx_62i.
Device speed data version:  PRODUCTION 1.27 2003-12-13.


Device utilization summary:

   Number of External IOBs            18 out of 140    12%
      Number of LOCed External IOBs    0 out of 18      0%





Overall effort level (-ol):   Standard (set by user)
Placer effort level (-pl):    Standard (set by user)
Placer cost table entry (-t): 1
Router effort level (-rl):    Standard (set by user)


Phase 1.1
Phase 1.1 (Checksum:989691) REAL time: 0 secs 

Phase 2.23
Phase 2.23 (Checksum:1312cfe) REAL time: 0 secs 

Phase 3.3
Phase 3.3 (Checksum:1c9c37d) REAL time: 0 secs 

Phase 4.5
Phase 4.5 (Checksum:26259fc) REAL time: 0 secs 

Phase 5.8
Phase 5.8 (Checksum:2faf07b) REAL time: 0 secs 

Phase 6.5
Phase 6.5 (Checksum:39386fa) REAL time: 0 secs 

Phase 7.18
Phase 7.18 (Checksum:42c1d79) REAL time: 0 secs 

Writing design to file counter.ncd.

Total REAL time to Placer completion: 0 secs 
Total CPU time to Placer completion: 0 secs 


Phase 1: 0 unrouted;       REAL time: 0 secs 

Phase 2: 0 unrouted;       REAL time: 0 secs 

Phase 3: 0 unrouted;       REAL time: 0 secs 

Phase 4: 0 unrouted;       REAL time: 0 secs 

Total REAL time to Router completion: 0 secs 
Total CPU time to Router completion: 0 secs 

Generating "par" statistics.


   The Delay Summary Report

   The SCORE FOR THIS DESIGN is: 0


The NUMBER OF SIGNALS NOT COMPLETELY ROUTED for this design is: 0

   The AVERAGE CONNECTION DELAY for this design is:        0.000
   The MAXIMUM PIN DELAY IS:                               0.000
   The AVERAGE CONNECTION DELAY on the 10 WORST NETS is:   0.000

   Listing Pin Delays by value: (nsec)

    d < 1.00   < d < 2.00  < d < 3.00  < d < 4.00  < d < 5.00  d >= 5.00
   ---------   ---------   ---------   ---------   ---------   ---------
           0           0           0           0           0           0

Generating Pad Report.

All signals are completely routed.

Total REAL time to PAR completion: 0 secs 
Total CPU time to PAR completion: 0 secs 

Peak Memory Usage:  44 MB

Placement: Completed - No errors found.
Routing: Completed - No errors found.

Writing design to file counter.ncd.


PAR done.
