iMPACT Version: G.28
iMPACT log file Started on 2005/07/23 19:03:52
// *** BATCH CMD : setPreference -pref UserLevel:NOVICE
// *** BATCH CMD : setPreference -pref MessageLevel:DETAILED
// *** BATCH CMD : setPreference -pref ConcurrentMode:FALSE
// *** BATCH CMD : setPreference -pref UseHighz:FALSE
// *** BATCH CMD : setPreference -pref ConfigOnFailure:STOP
// *** BATCH CMD : setPreference -pref StartupCLock:AUTO_CORRECTION
// *** BATCH CMD : setPreference -pref AutoSignature:FALSE
// *** BATCH CMD : setPreference -pref KeepSVF:FALSE
// *** BATCH CMD : setPreference -pref svfUseTime:FALSE
// *** BATCH CMD : setPreference -pref UserLevel:NOVICE
// *** BATCH CMD : setPreference -pref MessageLevel:DETAILED
// *** BATCH CMD : setPreference -pref ConcurrentMode:FALSE
// *** BATCH CMD : setPreference -pref UseHighz:FALSE
// *** BATCH CMD : setPreference -pref ConfigOnFailure:STOP
// *** BATCH CMD : setPreference -pref StartupCLock:AUTO_CORRECTION
// *** BATCH CMD : setPreference -pref AutoSignature:FALSE
// *** BATCH CMD : setPreference -pref KeepSVF:FALSE
// *** BATCH CMD : setPreference -pref svfUseTime:FALSE
// *** BATCH CMD : setMode -pff
// *** BATCH CMD : setMode -pff
// *** BATCH CMD : setMode -pff
// *** BATCH CMD : addConfigDevice -size 128 -name "xcf01s" -path "d:\engineering\work\naswi\xskripsi/"
// *** BATCH CMD : setSubmode -pffserial
// *** BATCH CMD : addPromDevice -position 1 -size -1 -name "xcf01s"
'1': Added Device xcf01s successfully.
----------------------------------------------------------------------
// *** BATCH CMD : setMode -pff
// *** BATCH CMD : setSubmode -pffserial
// *** BATCH CMD : setAttribute -configdevice -attr size -value "0"
// *** BATCH CMD : addCollection -name "av0"
// *** BATCH CMD : setAttribute -collection -attr dir -value "UP"
// *** BATCH CMD : addDesign -version 0 -name "0000"
// *** BATCH CMD : addDeviceChain -index 0
// *** BATCH CMD : addDevice -position 1 -file "D:\Engineering\Work\Naswi\xskripsi\top_level2.bit"
'1': Loading file 'D:\Engineering\Work\Naswi\xskripsi\top_level2.bit' ...
INFO:iMPACT - Elapsed time =      1 sec.
done.
INFO:iMPACT:501 - '1': Added Device xc2s50 successfully.
----------------------------------------------------------------------
----------------------------------------------------------------------
GUI --- Add one device.
// *** BATCH CMD : setMode -pff
Collection : av0
Design : 0
Device Chain : 0
----------------------------------------------------------------------
Position	PartName       	FileName            
1       	xc2s50         	D:\Engineering\Work\Naswi\xskripsi\top_level2.bit
----------------------------------------------------------------------
// *** BATCH CMD : setAttribute -configdevice -attr fillValue -value "FF"
// *** BATCH CMD : setAttribute -configdevice -attr fileFormat -value "mcs"
// *** BATCH CMD : setAttribute -collection -attr dir -value "UP"
// *** BATCH CMD : setAttribute -configdevice -attr path -value "d:\engineering\work\naswi\xskripsi/"
// *** BATCH CMD : setAttribute -collection -attr name -value "av0"
// *** BATCH CMD : generate
0x1110c (69900) bytes loaded up from 0x0
Using user-specified prom size of 128K
Writing file "d:\engineering\work\naswi\xskripsi//av0.mcs".
Writing file "d:\engineering\work\naswi\xskripsi//av0.prm".
Writing file "d:\engineering\work\naswi\xskripsi//av0.sig".
GUI --- Total configuration bit size = 559200 bits.
GUI --- Total configuration byte size = 69900 bytes.
GUI --- Switch to Configuration Mode
// *** BATCH CMD : setMode -bs
GUI --- Auto connect to cable...
// *** BATCH CMD : setCable -port auto
AutoDetecting cable. Please wait.
CB_PROGRESS_START - Starting Operation.
Connecting to cable (USB Port).
Cable connection failed.
Connecting to cable (Parallel Port - LPT1).
Checking cable driver.
 Driver windrvr6.sys version = 6.0.3.0. LPT base address = 0378h.
 ECP base address = FFFFFFFFh.
Cable connection established.
CB_PROGRESS_END - End Operation.
Elapsed time =      4 sec.
// *** BATCH CMD : Identify
PROGRESS_START - Starting Operation.
Identifying chain contents ....'1': : Manufacturer's ID =Xilinx xcf01s, Version : 0
INFO:iMPACT:1777 - 
Reading D:/Engineering/Xilinx6_2i/xcf/data/xcf01s.bsd...
Reading D:/Engineering/Xilinx6_2i/xcf/data/xcf01s.bsd...
INFO:iMPACT:501 - '1': Added Device xcf01s successfully.
----------------------------------------------------------------------
----------------------------------------------------------------------
'2': : Manufacturer's ID =Xilinx xc2s50, Version : 8
INFO:iMPACT:1777 - 
Reading D:/Engineering/Xilinx6_2i/spartan2/data/xc2s50.bsd...
Reading D:/Engineering/Xilinx6_2i/spartan2/data/xc2s50.bsd...
INFO:iMPACT:501 - '1': Added Device xc2s50 successfully.
----------------------------------------------------------------------
----------------------------------------------------------------------
done.
PROGRESS_END - End Operation.
Elapsed time =      3 sec.
// *** BATCH CMD : setAttribute -position 1 -attr configFileName -value "D:\Engineering\Work\Naswi\xskripsi\top_level2.bit"
'1': Loading file 'D:\Engineering\Work\Naswi\xskripsi\top_level2.bit' ...
done.
WARNING:iMPACT:1049 - Startup Clock has been changed to 'JtagClk' in the bitstream stored in memory,
but the original bitstream file remains unchanged.
but the original bitstream file remains unchanged.
INFO:iMPACT:501 - '1': Added Device xc2s50 successfully.
----------------------------------------------------------------------
----------------------------------------------------------------------
----------------------------------------------------------------------
----------------------------------------------------------------------
xc18v01_pc20
xc18v01_so20
xc18v01_vq44
xc18v02_pc44
xc18v02_vq44
xc18v04_pc44
xc18v04_vq44
xcf01s_vo20
xcf02s_vo20
xcf04s_vo20
xcf08p_fs48
xcf32p_fs48
xcf32p_vo48
// *** BATCH CMD : setAttribute -position 2 -attr devicePartName -value "xcf01s"
// *** BATCH CMD : setAttribute -position 2 -attr configFileName -value "D:\Engineering\Work\Naswi\xskripsi\av0.mcs"
'2': Loading file 'D:\Engineering\Work\Naswi\xskripsi\av0.mcs' ...
done.
// *** BATCH CMD : Program -p 2 -e -v -loadfpga 
PROGRESS_START - Starting Operation.
Validating chain...
Boundary-scan chain validated successfully.
'2': Putting device in ISP mode...done.
'2': Erasing device...done.
'2': Erasure completed successfully.
'2': Putting device in ISP mode...done.
'2': Programming device...done.
'2': Putting device in ISP mode...done.
'2': Putting device in ISP mode...done.
'2': Verifying device...done.
'2': Verification completed successfully.
'2': Calculated checksum matches expected checksum, 0012a64de
'2': Putting device in ISP mode...done.
'2': Setting user-programmable bits...
done.
'2': Putting device in ISP mode...done.
'2': Starting FPGA Load with Prom Data...INFO:iMPACT:563 - '2':Please ensure proper connections as specified by the data book ...
'2': Programming completed successfully.
PROGRESS_END - End Operation.
Elapsed time =     25 sec.
// *** BATCH CMD : setMode -pff
// *** BATCH CMD : setAttribute -configdevice -attr fileFormat -value "mcs"
// *** BATCH CMD : setAttribute -configdevice -attr swapBit -value "FALSE"
// *** BATCH CMD : setAttribute -configdevice -attr fillValue -value "FF"
// *** BATCH CMD : setAttribute -collection -attr dir -value "UP"
// *** BATCH CMD : setMode -sm
// *** BATCH CMD : setMode -bs
// *** BATCH CMD : setMode -bs
// *** BATCH CMD : setMode -ss
Cable output is not connected. Please select the desired output cable.
// *** BATCH CMD : setMode -sm
Cable output is not connected. Please select the desired output cable.
// *** BATCH CMD : setMode -bsfile
Cable output is not connected. Please select the desired output cable.
// *** BATCH CMD : setMode -dtconfig
Cable output is not connected. Please select the desired output cable.
// *** BATCH CMD : setMode -cf
// *** BATCH CMD : setMode -mpm
// *** BATCH CMD : setMode -pff
// *** BATCH CMD : setMode -bs
// *** BATCH CMD : setMode -bs
*****   Closing iMPACT program.   *****
----------------------------------------------------------------------
----------------------------------------------------------------------
