Power Report

Release 6.2i - XPower SoftwareVersion:G.28
Copyright (c) 1995-2004 Xilinx, Inc. All rights reserved.

Design: | pid_sysgen_clk_wrapper
Preferences: | pid_sysgen_clk_wrapper.pcf
Part: | 2s50pq208-6
Data version: | PRELIMINARY,v1.0,07-31-02

Power summary: | I(mA) | P(mW)
Total estimated power consumption: |  | 19
Vccint 2.50V: | 5 | 12
Vcco33 3.30V: | 2 | 7
Clocks: | 3 | 7
Inputs: | 0 | 1
Logic: | 0 | 0
Outputs: |  |
Vcco33 | 0 | 0
Signals: | 0 | 0
Quiescent Vccint 2.50V: | 2 | 5
Quiescent Vcco33 3.30V: | 2 | 7

Thermal summary: |
Estimated junction temperature: | 26C
Ambient temp: | 25C
Case temp: | 26C
Theta J-A range: | 34 - 35C/W

Decoupling Network Summary: | Cap Range (uF) | #
Capacitor Recommendations: |  |
Total for Vccint |  | 12
| 470.0-1000.0 | 1
| 0.470- 2.200 | 1
| 0.0470-0.2200 | 2
| 0.0100-0.0470 | 3
| 0.0010-0.0047 | 5
Total for Vcco33 |  | 6
| 470.0-1000.0 | 1
| 0.0470-0.2200 | 1
| 0.0100-0.0470 | 1
| 0.0010-0.0047 | 3

Analysis completed: Mon Apr 11 01:05:43 2005