#PACE: Start of Constraints generated by PACE

#PACE: Start of PACE I/O Pin Assignments
NET "anode0"  LOC = "P60"  ;
NET "anode1"  LOC = "P69"  ;
NET "anode2"  LOC = "P71"  ;
NET "anode3"  LOC = "P75"  ;
NET "cathode<0>"  LOC = "P46"  ;
NET "cathode<1>"  LOC = "P45"  ;
NET "cathode<2>"  LOC = "P44"  ;
NET "cathode<3>"  LOC = "P43"  ;
NET "cathode<4>"  LOC = "P42"  ;
NET "cathode<5>"  LOC = "P41"  ;
NET "cathode<6>"  LOC = "P37"  ;
NET "cathode<7>"  LOC = "P36"  ;
NET "ce_sg_n"  LOC = "P58"  ;
NET "clk_sg"  LOC = "P77"  ;
NET "in_x_0<0>"  LOC = "P206"  ;
NET "in_x_0<10>"  LOC = "P82"  ;
NET "in_x_0<11>"  LOC = "P81"  ;
NET "in_x_0<12>"  LOC = "P202"  ;
NET "in_x_0<13>"  LOC = "P201"  ;
NET "in_x_0<14>"  LOC = "P200"  ;
NET "in_x_0<15>"  LOC = "P199"  ;
NET "in_x_0<1>"  LOC = "P205"  ;
NET "in_x_0<2>"  LOC = "P204"  ;
NET "in_x_0<3>"  LOC = "P203"  ;
NET "in_x_0<4>"  LOC = "P89"  ;
NET "in_x_0<5>"  LOC = "P88"  ;
NET "in_x_0<6>"  LOC = "P87"  ;
NET "in_x_0<7>"  LOC = "P86"  ;
NET "in_x_0<8>"  LOC = "P84"  ;
NET "in_x_0<9>"  LOC = "P83"  ;
NET "reset"  LOC = "P59"  ;

#PACE: Start of PACE Area Constraints

#PACE: Start of PACE Prohibit Constraints

#PACE: End of Constraints generated by PACE
